|  |
| --- |
| **PANEL SCHEDULE** |

|  |  |  |
| --- | --- | --- |
| **General Information** | | **Breaker Details** |
| **Panel ID** | [ID Number] | Main Breaker [Rate] Amp |
| **Panel Location** | [Location] | Main Lugs Only |
| **Fed From** | [Number] | Fed-thru Lugs |

|  |  |  |
| --- | --- | --- |
| **Phase Type** | **Voltage Type** | |
| Single Phase | 120 / 240 | 120 / 208 |
| Three Phase | 277/ 480 |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Breaker** | **Pole** | **Wire (AWG)** | **Pipe Size** | **VA** | **Voltage** | **Description** | **Circuit** |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

**Notes**

1) All Electrical Works Shall Be Done In Accordance With The Approved Drawings, The National Electrical Code And Current Local Electricity Laws And Regulations. Any Deviation From The Approved Drawings Shall First Be Approved By The Electrical Inspectorate. 2) All Electrical Works Is To Be Done In A Neat And Acceptable Manner. 3) Provide 4-Wire Branch Circuits For All Dryers, Ranges And Cook Tops. 4) All Switches / Receptacles Located In Bath Rooms To Have Ground Fault Protection. 5) No Mini Breakers Are To Be Installed 6) Provide Light And Receptacle In Attic For Servicing Equipment.