|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **Mileage** | **PM "A"** | **PM "B"** | **Service Details** | **Serviced By** | **LabourCost** | **MaterialCost** | **TOTAL** |
| 10/01/2020 | 5,200 |  |  | PM "A" + Front left light change | Truck Service 1 | $145.00 | $15.00 | **$160.00** |
| 20/04/2020 | 9,150 |  |  | Right door handle replaced | Truck Service 2 | $40.00 | $75.00 | **$115.00** |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |

**Truck Maintenance Log**

**PM "A"** PREVENTIVE MAINTENANCE also known as a “safety inspection” consists of a safety check and lubrication as well as checks of key components such as brakes, lights, tire condition and inflation, and fluids. It also includes checking and adjusting high-wear components. The normal interval for “A” service is between 5,000 and 10,000 miles.

**PM "B"** PREVENTIVE MAINTENANCE normally includes all PM A items, and also include an oil and filter change as well as more in-depth checks of the engine and driveline. The normal interval for “B” service is 10,000 to 20,000 miles. A PM B should also include a download of the ECM and action on any trouble codes or problems reported by the ECM (if applicable).